## Преглед на менютата

Контролният панел предоставя достъп до разнообразни менюта с цел да се настрои принтерът или да се използват функциите на принтера.

- Тази функция не се поддържа за SCX-340x/SCX-340xW Series (вж. Преглед на контролния панел).

- Възможно е някои менюта да не се извеждат на дисплея, в зависимост от опциите или моделите. Ако това се случи, съответната опция не е налична за вашето устройство.

- Някои имена на менюта може да се различават от тези на вашето устройство, в зависимост от неговите опции или модели.

- Менютата са описани в Разширеното ръководство (вж. Менюта с полезни настройки).

### Достъп до менюто

1. Изберете бутона "Факс", "Копиране" или "Сканиране" върху панела за управление в зависимост от функцията, която ще бъде използвана.

2. Изберете (Menu), докато желаното от Вас меню се изведе в най-долния ред на дисплея, след което натиснете OK.

3. Натискайте стрелките, докато желаният елемент на менюто се появи и натиснете OK.

4. Ако елементът за настройка съдържа и подменюта, повторете стъпка 3.

5. Натиснете OK, за да запазите избора си.

6. Натиснете (Stop/Clear), за да се върнете в режим на готовност.

Елементи | Опции
--- | ---
Fax Feature | Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Resolution | Standard Fine Super Fine Photo Fax Color Fax
Scan Size
Multi Send
Delay Send
Fax Feature (Продължение) | Priority Send
Forward | Fax PC
Secure Receive | Off On Print
Add Page
Cancel Job

Fax Setup

Sending

Redial Times

Redial Term

Prefix Dial

ECM Mode

Send Report

Image TCR

Dial Mode [a]

Fax Setup (Продължение)

Receiving

Receive Mode

Ring To Answer

Stamp RCV Name

RCV Start Code

Auto Reduction

Discard Size

Junk Fax Setup

DRPD Mode [a]

Change Default | Resolution Darkness Contrast Scan Size
Auto Report | On Off
Copy Feature | Scan Size
Reduce/Enlarge
Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Copy Feature (Продължи) | Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Original Type | Text Text/Photo Photo

Layout

Normal

2-Up

4-Up

ID Copy

Poster Copy

Clone Copy

Adjust Bkgd. | Off Auto Enhance Lev.1 Enhance Lev.2 Erase Lev.1- Erase Lev.4

Copy Setup

Change Default

Scan Size

Copies

Copy Collation

Reduce/Enlarge

Darkness

Contrast

Original Type

Adjust Bkgd.

System Setup

Machine Setup

Machine ID

Fax Number

Date & Time

Clock Mode

Language

Power Save

Wakeup Event

System Timeout

Altitude Adj.

Auto Continue [b]

Paper Mismatch

Paper Substit. [b]

Toner Save

Eco Settings

Paper Setup | Paper Size Paper Type Margin
System Setup (Продължение) | Sound/Volume | Key Sound Alarm Sound Speaker Ringer

Report

All Report

Configuration

Supplies Info.

Address Book

Fax Send

Fax Sent

Fax Received

Schedule Jobs

Junk Fax

Network Conf. [c]

Usage Counter

Fax Options

Maintenance | CLR Empty Msg. [d] Supplies Life Serial No. TonerLow Alert

System Setup (Продължение)

Clear Setting

All Settings

Fax Setup

Copy Setup

System Setup

Network Setup [c]

Address Book

Fax Sent

Fax Received

Network [c] | TCP/IP (IPv4) | DHCP BOOTP Static
TCP/IP (IPv6) | IPv6 Activate DHCPv6 Config
Ethernet Speed | Automatic 10Mbps Half 10Mbps Full 100Mbps Half 100Mbps Full

Network [c] (Продължава)

Wireless

Wi-Fi ON/OFF

Wi-Fi Direct

WPS Setting

WLAN Setting

WLAN Default

WLAN Signal

Clear Setting
Network Conf.
[a] Тази опция може да не е налична, в зависимост от страната ви. [b] Опцията се появява само ако е разрешено Paper Mismatch. [c] Само SCX-340xFW/SCX-340xHW Series. [d] Тази опция се появява, само когато в касетата е останало малко количество тонер.