## Pregled menija

Nadzorna plošča omogoča dostop do različnih menijev, v katerih lahko nastavite napravo ali uporabite njene funkcije.

- Ta funkcija ni na voljo za SCX-340x/SCX-340xW Series (glejte Pregled nadzorne plošče).

- Prikaz menijev na zaslonu je odvisen od možnosti in modela. V tem primeru jih v napravi ni mogoče uporabljati.

- Nekatera imena menijev se lahko razlikujejo od tistih na vaši napravi, odvisno od možnosti ali modelov.

- Meniji so opisani v Advanced Guide (glejte Uporabni nastavitveni meniji).

### Odpiranje menija

1. Na nadzorni plošči izberite gumb za pošiljanje faksov, kopiranje ali obtično branje , odvisno od želene funkcije.

2. Pritiskajte (Menu) dokler se na dnu zaslona ne prikaže želeni meni, nato pa pritisnite OK.

3. S puščicami se pomikajte dokler se na meniju ne izpiše želeni element in nato pritisnite OK.

4. Če ima element nastavitve podmenije, ponovite 3. korak.

5. Če želite shraniti izbiro, pritisnite OK.

6. Pritisnite (Stop/Clear) za vrnitev v stanje pripravljenosti.

Zadeve | Možnosti
--- | ---
Fax Feature | Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Resolution | Standard Fine Super Fine Photo Fax Color Fax
Scan Size
Multi Send
Delay Send
Fax Feature (nadaljuj) | Priority Send
Forward | Fax PC
Secure Receive | Off On Print
Add Page
Cancel Job

Fax Setup

Sending

Redial Times

Redial Term

Prefix Dial

ECM Mode

Send Report

Image TCR

Dial Mode [a]

Fax Setup (nadaljuj)

Receiving

Receive Mode

Ring To Answer

Stamp RCV Name

RCV Start Code

Auto Reduction

Discard Size

Junk Fax Setup

DRPD Mode [a]

Change Default | Resolution Darkness Contrast Scan Size
Auto Report | On Off
Copy Feature | Scan Size
Reduce/Enlarge
Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Copy Feature (naprej) | Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Original Type | Text Text/Photo Photo

Layout

Normal

2-Up

4-Up

ID Copy

Poster Copy

Clone Copy

Adjust Bkgd. | Off Auto Enhance Lev.1 Enhance Lev.2 Erase Lev.1- Erase Lev.4

Copy Setup

Change Default

Scan Size

Copies

Copy Collation

Reduce/Enlarge

Darkness

Contrast

Original Type

Adjust Bkgd.

System Setup

Machine Setup

Machine ID

Fax Number

Date & Time

Clock Mode

Language

Power Save

Wakeup Event

System Timeout

Altitude Adj.

Auto Continue [b]

Paper Mismatch

Paper Substit. [b]

Toner Save

Eco Settings

Paper Setup | Paper Size Paper Type Margin
System Setup (nadaljuj) | Sound/Volume | Key Sound Alarm Sound Speaker Ringer

Report

All Report

Configuration

Supplies Info.

Address Book

Fax Send

Fax Sent

Fax Received

Schedule Jobs

Junk Fax

Network Conf. [c]

Usage Counter

Fax Options

Maintenance | CLR Empty Msg. [d] Supplies Life Serial No. TonerLow Alert

System Setup (nadaljuj)

Clear Setting

All Settings

Fax Setup

Copy Setup

System Setup

Network Setup [c]

Address Book

Fax Sent

Fax Received

Network [c] | TCP/IP (IPv4) | DHCP BOOTP Static
TCP/IP (IPv6) | IPv6 Activate DHCPv6 Config
Ethernet Speed | Automatic 10Mbps Half 10Mbps Full 100Mbps Half 100Mbps Full

Network [c] (naprej)

Wireless

Wi-Fi ON/OFF

Wi-Fi Direct

WPS Setting

WLAN Setting

WLAN Default

WLAN Signal

Clear Setting
Network Conf.
[a] Ta možnost morda ni na voljo v vseh državah. [b] Ta opcija se pojavi samo, ko je aktivirana funkcija Paper Mismatch. [c] samo SCX-340xFW/SCX-340xHW Series. [d] Ta možnost se pojavi le, ko je v kartuši le še malo črnila.