e3c2efce: ndt_1c Msg: Querying if miniport is wireless
e3c2efce: ndt_1c Msg: Miniport AX887721 is ** NOT Wireless-LAN **
<TESTGROUP>

*** ==================================================================
*** SUITE INFORMATION
***
*** Suite Name:        N/A (built on the fly)
*** Suite Description: N/A
*** Number of Tests:   13
*** ==================================================================

*** ==================================================================
*** SYSTEM INFORMATION
***
*** Date and Time:          05/26/2010 10:00 AM (Wednesday)
***
*** Device Name:            CEPC
***
*** OS Version:             5.0
*** Build Number:           1400
*** Platform ID:            3 "Windows CE"
*** Version String:         ""
***
*** Processor Type:         0x000002AE (686) "Intel Pentium II"
*** Processor Architecture: 0x0000     (0) "Intel"
*** Page Size:              0x00001000 (4,096)
*** Minimum App Address:    0x00010000 (65,536)
*** Maximum App Address:    0x7FFFFFFF (2,147,483,647)
*** Active Processor Mask:  0x00000001
*** Number Of Processors:   1
*** Allocation Granularity: 0x00010000 (65,536)
*** Processor Level:        0x0003     (3)
*** Processor Revision:     0x0004     (4)
*** ==================================================================

*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:    24,092,672 bytes
*** Memory Used:      5,689,344 bytes
*** Memory Free:     18,403,328 bytes
***
*** Kernel Used:        544,768 bytes
*** Water Mark:           4,492 pages
***
*** Store Total:     24,027,136 bytes
*** Store Used:         570,992 bytes
*** Store Free:      23,456,144 bytes
*** ==================================================================

BEGIN GROUP: ndt_1c.dll
<TESTCASE ID=1>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_OpenClose
*** Test ID:        1
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    20787
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_OpenClose", Threads=0, Seed=20787
      e3c2efce: ndt_1c Msg: Start 1c_OpenClose test on the adapter AX887721
      e3c2efce: ndt_1c Msg: Opening adapter
      e3c2efce: ndt_1c Msg: Repeatedly binding and unbinding the adapter
      e3c2efce: ndt_1c Msg: Open and bind the adapter multiple times, then close each open instance
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #0)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #1)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #2)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #3)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #4)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #5)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #6)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #7)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #8)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #9)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #10)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #11)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #12)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #13)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #14)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Opening 128 adapter instances (pass #15)
      e3c2efce: ndt_1c Msg: Closing all adapter instances
      e3c2efce: ndt_1c Msg: Test 1c_OpenClose on the adapter AX887721 PASS
   END TEST: "1c_OpenClose", PASSED, Time=8.829
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_OpenClose
*** Test ID:        1
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    20787
*** Thread Count:   1
*** Execution Time: 0:00:08.829
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=2>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_Send
*** Test ID:        2
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    2384
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_Send", Threads=0, Seed=2384
      e3c2efce: ndt_1c Msg: Start 1c_Send test on the adapter AX887721
      e3c2efce: ndt_1c Msg: Getting basic info about the adapter
      e3c2efce: ndt_1c Msg: Get OID_GEN_MAXIMUM_TOTAL_SIZE = 1514
      e3c2efce: ndt_1c Msg: Get OID_GEN_MAXIMUM_FRAME_SIZE = 1500
      e3c2efce: ndt_1c Msg: Testing sending to a (random) directed address
      e3c2efce: ndt_1c Msg: Sending: Send
      e3c2efce: ndt_1c Msg: Sending to a random address
      e3c2efce: ndt_1c Msg: Sending: Send
      e3c2efce: ndt_1c Msg: Sending to a broadcast address
      e3c2efce: ndt_1c Msg: Sending: Send
      e3c2efce: ndt_1c Msg: Sending to a multicast/functional address
      e3c2efce: ndt_1c Msg: Sending: Send
      e3c2efce: ndt_1c Msg: Testing sending to a group of addresses
   END TEST: "1c_Send", PASSED, Time=49.439
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_Send
*** Test ID:        2
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    2384
*** Thread Count:   1
*** Execution Time: 0:00:49.439
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=3>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_LoopbackSend
*** Test ID:        3
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    7823
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_LoopbackSend", Threads=0, Seed=7823
      e3c2efce: ndt_1c Msg: Start 1c_Loopback test
      e3c2efce: ndt_1c Msg: The test adapter is AX887721
      e3c2efce: ndt_1c Msg: Opening adapters
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Get basic adapter info
      e3c2efce: ndt_1c Msg: Possible filter settings:
      e3c2efce: ndt_1c Msg:   - Directed
      e3c2efce: ndt_1c Msg:   - Broadcast
      e3c2efce: ndt_1c Msg:   - Promiscuous
      e3c2efce: ndt_1c Msg:   - Multicast
      e3c2efce: ndt_1c Msg:   - All Multicast
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 2 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 2 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 2 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 2 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 2 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 2 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 2 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 2 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 2 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 3 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 2 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 3 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 2 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 3 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 2 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 3 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 2 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 3 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 1 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 2 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 1 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 2 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 1 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 2 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 2 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 3 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 1 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 2 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 3 properly didn't receive packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 1 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 2 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Setting receiving filters
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      e3c2efce: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      e3c2efce: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      e3c2efce: ndt_1c Msg: Stop receiving and checking results
      e3c2efce: ndt_1c Msg: Instance 0 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 1 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 2 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 3 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 4 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 5 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 6 received expected 300 packets
      e3c2efce: ndt_1c Msg: Instance 7 received expected 300 packets
      e3c2efce: ndt_1c Msg: Unbinding adapters
   END TEST: "1c_LoopbackSend", PASSED, Time=291.052
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_LoopbackSend
*** Test ID:        3
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    7823
*** Thread Count:   1
*** Execution Time: 0:04:51.052
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=4>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_LoopbackStress
*** Test ID:        4
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    25585
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_LoopbackStress", Threads=0, Seed=25585
      e3c2efce: ndt_1c Msg: Start 1c_LoopbackStess test on the adapter AX887721
      e3c2efce: ndt_1c Msg: Getting informations about the adapter
      e3c2efce: ndt_1c Msg: Opening adapters
      e3c2efce: ndt_1c Msg: Start Stress Tests
      e3c2efce: ndt_1c Msg: Test #0
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Start sending
      e3c2efce: ndt_1c Msg: Wait to finish with sending
      e3c2efce: ndt_1c Msg: Stop listening
      e3c2efce: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7735354 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7735354 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Test #1
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Start sending
      e3c2efce: ndt_1c Msg: Wait to finish with sending
      e3c2efce: ndt_1c Msg: Stop listening
      e3c2efce: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7785021 bytes in 12491 ms
      e3c2efce: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12491 ms
      e3c2efce: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7785021 bytes in 12491 ms
      e3c2efce: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12491 ms
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Test #2
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Start sending
      e3c2efce: ndt_1c Msg: Wait to finish with sending
      e3c2efce: ndt_1c Msg: Stop listening
      e3c2efce: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7806724 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7806724 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Test #3
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Start sending
      e3c2efce: ndt_1c Msg: Wait to finish with sending
      e3c2efce: ndt_1c Msg: Stop listening
      e3c2efce: ndt_1c Msg: Bind #0: Sent 100 packets with total size 9650 bytes in 120 ms
      e3c2efce: ndt_1c Msg: Bind #0: Recv 100 packets with total size 4600 bytes in 120 ms
      e3c2efce: ndt_1c Msg: Bind #1: Recv 100 packets with total size 9650 bytes in 120 ms
      e3c2efce: ndt_1c Msg: Bind #1: Sent 100 packets with total size 4600 bytes in 120 ms
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Test #4
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Start sending
      e3c2efce: ndt_1c Msg: Wait to finish with sending
      e3c2efce: ndt_1c Msg: Stop listening
      e3c2efce: ndt_1c Msg: Bind #0: Sent 53 packets with total size 3869 bytes in 60 ms
      e3c2efce: ndt_1c Msg: Bind #0: Recv 53 packets with total size 3869 bytes in 60 ms
      e3c2efce: ndt_1c Msg: Bind #1: Recv 53 packets with total size 3869 bytes in 60 ms
      e3c2efce: ndt_1c Msg: Bind #1: Sent 53 packets with total size 3869 bytes in 60 ms
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Test #5
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Start sending
      e3c2efce: ndt_1c Msg: Wait to finish with sending
      e3c2efce: ndt_1c Msg: Stop listening
      e3c2efce: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 1140000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 1140000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Test #6
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Start sending
      e3c2efce: ndt_1c Msg: Wait to finish with sending
      e3c2efce: ndt_1c Msg: Stop listening
      e3c2efce: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7757383 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7757383 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Test #7
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Start sending
      e3c2efce: ndt_1c Msg: Wait to finish with sending
      e3c2efce: ndt_1c Msg: Stop listening
      e3c2efce: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7837313 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7837313 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Sent 0 packets with total size 0 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Test #8
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Start sending
      e3c2efce: ndt_1c Msg: Wait to finish with sending
      e3c2efce: ndt_1c Msg: Stop listening
      e3c2efce: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7879771 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 7879771 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7879771 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 7879771 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Test #9
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Start sending
      e3c2efce: ndt_1c Msg: Wait to finish with sending
      e3c2efce: ndt_1c Msg: Stop listening
      e3c2efce: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 740000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 740000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 740000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 740000 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Start simultaneous stress tests
      e3c2efce: ndt_1c Msg: Binding to adapters
      e3c2efce: ndt_1c Msg: Start receiving
      e3c2efce: ndt_1c Msg: Start sending
      e3c2efce: ndt_1c Msg: Wait to finish with sending
      e3c2efce: ndt_1c Msg: Stop listening
      e3c2efce: ndt_1c Msg: Bind #0: Sent 6 packets with total size 297 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #0: Recv 6 packets with total size 297 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Sent 6 packets with total size 297 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #1: Recv 6 packets with total size 297 bytes in 12490 ms
      e3c2efce: ndt_1c Msg: Bind #2: Sent 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Bind #2: Recv 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Bind #3: Sent 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Bind #3: Recv 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Bind #4: Recv 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Bind #4: Sent 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Bind #5: Recv 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Bind #5: Sent 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Bind #6: Recv 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Bind #6: Sent 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Bind #7: Recv 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Bind #7: Sent 6 packets with total size 297 bytes in 0 ms
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Closing adapters
   END TEST: "1c_LoopbackStress", PASSED, Time=125.610
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_LoopbackStress
*** Test ID:        4
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    25585
*** Thread Count:   1
*** Execution Time: 0:02:05.610
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=5>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_SetMulticast
*** Test ID:        5
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    18052
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_SetMulticast", Threads=0, Seed=18052
      e3c2efce: ndt_1c Msg: Start 1c_SetMulticast test
      e3c2efce: ndt_1c Msg: The test adapter is AX887721
      e3c2efce: ndt_1c Msg: Opening adapters
      e3c2efce: ndt_1c Msg: Binding to adapters
      e3c2efce: ndt_1c Msg: GetMaxListSize
      e3c2efce: ndt_1c Msg: Driver support 64 address in multicast list
      e3c2efce: ndt_1c Msg: 64 multicast addresses will be tested
      e3c2efce: ndt_1c Msg: Add/Delete a multicast address multiple times
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add as many multicast addresses as driver says it supports
      e3c2efce: ndt_1c Msg: Adding multicast address 1
      e3c2efce: ndt_1c Msg: Adding multicast address 2
      e3c2efce: ndt_1c Msg: Adding multicast address 3
      e3c2efce: ndt_1c Msg: Adding multicast address 4
      e3c2efce: ndt_1c Msg: Adding multicast address 5
      e3c2efce: ndt_1c Msg: Adding multicast address 6
      e3c2efce: ndt_1c Msg: Adding multicast address 7
      e3c2efce: ndt_1c Msg: Adding multicast address 8
      e3c2efce: ndt_1c Msg: Adding multicast address 9
      e3c2efce: ndt_1c Msg: Adding multicast address 10
      e3c2efce: ndt_1c Msg: Adding multicast address 11
      e3c2efce: ndt_1c Msg: Adding multicast address 12
      e3c2efce: ndt_1c Msg: Adding multicast address 13
      e3c2efce: ndt_1c Msg: Adding multicast address 14
      e3c2efce: ndt_1c Msg: Adding multicast address 15
      e3c2efce: ndt_1c Msg: Adding multicast address 16
      e3c2efce: ndt_1c Msg: Adding multicast address 17
      e3c2efce: ndt_1c Msg: Adding multicast address 18
      e3c2efce: ndt_1c Msg: Adding multicast address 19
      e3c2efce: ndt_1c Msg: Adding multicast address 20
      e3c2efce: ndt_1c Msg: Adding multicast address 21
      e3c2efce: ndt_1c Msg: Adding multicast address 22
      e3c2efce: ndt_1c Msg: Adding multicast address 23
      e3c2efce: ndt_1c Msg: Adding multicast address 24
      e3c2efce: ndt_1c Msg: Adding multicast address 25
      e3c2efce: ndt_1c Msg: Adding multicast address 26
      e3c2efce: ndt_1c Msg: Adding multicast address 27
      e3c2efce: ndt_1c Msg: Adding multicast address 28
      e3c2efce: ndt_1c Msg: Adding multicast address 29
      e3c2efce: ndt_1c Msg: Adding multicast address 30
      e3c2efce: ndt_1c Msg: Adding multicast address 31
      e3c2efce: ndt_1c Msg: Adding multicast address 32
      e3c2efce: ndt_1c Msg: Adding multicast address 33
      e3c2efce: ndt_1c Msg: Adding multicast address 34
      e3c2efce: ndt_1c Msg: Adding multicast address 35
      e3c2efce: ndt_1c Msg: Adding multicast address 36
      e3c2efce: ndt_1c Msg: Adding multicast address 37
      e3c2efce: ndt_1c Msg: Adding multicast address 38
      e3c2efce: ndt_1c Msg: Adding multicast address 39
      e3c2efce: ndt_1c Msg: Adding multicast address 40
      e3c2efce: ndt_1c Msg: Adding multicast address 41
      e3c2efce: ndt_1c Msg: Adding multicast address 42
      e3c2efce: ndt_1c Msg: Adding multicast address 43
      e3c2efce: ndt_1c Msg: Adding multicast address 44
      e3c2efce: ndt_1c Msg: Adding multicast address 45
      e3c2efce: ndt_1c Msg: Adding multicast address 46
      e3c2efce: ndt_1c Msg: Adding multicast address 47
      e3c2efce: ndt_1c Msg: Adding multicast address 48
      e3c2efce: ndt_1c Msg: Adding multicast address 49
      e3c2efce: ndt_1c Msg: Adding multicast address 50
      e3c2efce: ndt_1c Msg: Adding multicast address 51
      e3c2efce: ndt_1c Msg: Adding multicast address 52
      e3c2efce: ndt_1c Msg: Adding multicast address 53
      e3c2efce: ndt_1c Msg: Adding multicast address 54
      e3c2efce: ndt_1c Msg: Adding multicast address 55
      e3c2efce: ndt_1c Msg: Adding multicast address 56
      e3c2efce: ndt_1c Msg: Adding multicast address 57
      e3c2efce: ndt_1c Msg: Adding multicast address 58
      e3c2efce: ndt_1c Msg: Adding multicast address 59
      e3c2efce: ndt_1c Msg: Adding multicast address 60
      e3c2efce: ndt_1c Msg: Adding multicast address 61
      e3c2efce: ndt_1c Msg: Adding multicast address 62
      e3c2efce: ndt_1c Msg: Adding multicast address 63
      e3c2efce: ndt_1c Msg: Adding multicast address 64
      e3c2efce: ndt_1c Msg: Delete all these added multicast addresses
      e3c2efce: ndt_1c Msg: Add/Delete a multicast address multiple times on two instances
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add/Query Multicast
      e3c2efce: ndt_1c Msg: Delete/Query Multicast
      e3c2efce: ndt_1c Msg: Add half of the maximum list size multicast address to each open instance
      e3c2efce: ndt_1c Msg: Delete all these added multicast addresses
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Closing adapters
   END TEST: "1c_SetMulticast", PASSED, Time=3.427
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_SetMulticast
*** Test ID:        5
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    18052
*** Thread Count:   1
*** Execution Time: 0:00:03.427
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=6>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_Reset
*** Test ID:        6
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    26220
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_Reset", Threads=0, Seed=26220
      e3c2efce: ndt_1c Msg: Start 1c_Reset test on the adapter AX887721
      e3c2efce: ndt_1c Msg: Opening adapters
      e3c2efce: ndt_1c Msg: Getting basic info about the adapter
      e3c2efce: ndt_1c Msg: Querying if miniport is wireless
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Sending packets
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Reset
      e3c2efce: ndt_1c Msg: Querying connect status
      e3c2efce: ndt_1c Msg: Unbinding adapters
      e3c2efce: ndt_1c Msg: Closing adapters
   END TEST: "1c_Reset", PASSED, Time=180.662
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_Reset
*** Test ID:        6
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    26220
*** Thread Count:   1
*** Execution Time: 0:03:00.662
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=7>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_CancelSend
*** Test ID:        7
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    20126
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_CancelSend", Threads=0, Seed=20126
      e3c2efce: ndt_1c Msg: Start 1c_CancelSend test on the adapter AX887721
      e3c2efce: ndt_1c Msg: Opening adapters
      e3c2efce: ndt_1c Msg: Getting basic info about the adapter
      e3c2efce: ndt_1c Msg: Binding adapters
      e3c2efce: ndt_1c Msg: Sending and cancel packets
      e3c2efce: ndt_1c Msg: Unbind adapters
      e3c2efce: ndt_1c Msg: 1000 packets was sent. 900 packet wasn't canceled. 0 packet was.
      e3c2efce: ndt_1c Msg: Closing adapters
   END TEST: "1c_CancelSend", PASSED, Time=6.485
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_CancelSend
*** Test ID:        7
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    20126
*** Thread Count:   1
*** Execution Time: 0:00:06.485
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=8>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_FaultHandling
*** Test ID:        8
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    225
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_FaultHandling", Threads=0, Seed=225
   END TEST: "1c_FaultHandling", SKIPPED, Time=0.000
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_FaultHandling
*** Test ID:        8
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Skipped
*** Random Seed:    225
*** Thread Count:   1
*** Execution Time: 0:00:00.000
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="SKIPPED">
<TESTCASE ID=9>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_OIDs
*** Test ID:        9
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    773
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_OIDs", Threads=0, Seed=773
      e3c2efce: ndt_1c Msg: Start 1c_TestOidsDeviceIoControl test on the adapter AX887721
      e3c2efce: ndt_1c Msg: Open adapter
      e3c2efce: ndt_1c Msg: Bind to adapter
      e3c2efce: ndt_1c Msg: Get Supported OIDs List
      e3c2efce: ndt_1c Msg: Check for all required OIDs
      e3c2efce: ndt_1c Msg: Check that listed OIDs really are supported
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010101 should be queried
      e3c2efce: ndt_1c Msg: The OID 0x00010101 was skippen
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010102 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010103 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010104 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010114 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010105 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010106 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010111 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010115 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010113 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010112 should be queried
      e3c2efce: ndt_1c Msg: The OID 0x00010112 was skippen
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010107 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010108 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x0001010a should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x0002020e should be queried
      e3c2efce: ndt_1c Msg: The OID 0x0002020e isn't required, and hence not checked
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010109 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x0001010b should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x0001010c should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x0001010d should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010116 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x0001010e should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x0001010f should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010110 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00020101 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00020103 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00020102 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00020104 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00020105 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x01010101 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x01010102 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x01010103 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x01010104 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x01020101 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x01020102 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x01020103 should be queried
      e3c2efce: ndt_1c Msg: Checking if an OID 0x00010117 should be queried
      e3c2efce: ndt_1c Msg: The OID 0x00010117 isn't required, and hence not checked
      e3c2efce: ndt_1c Msg: Checking if an OID 0xfd010100 should be queried
      e3c2efce: ndt_1c Msg: The OID 0xfd010100 isn't required, and hence not checked
      e3c2efce: ndt_1c Msg: Checking if an OID 0xfd010106 should be queried
      e3c2efce: ndt_1c Msg: The OID 0xfd010106 was skippen
      e3c2efce: ndt_1c Msg: Checking if an OID 0xfd010102 should be queried
      e3c2efce: ndt_1c Msg: The OID 0xfd010102 was skippen
      e3c2efce: ndt_1c Msg: Checking if an OID 0xfd010101 should be queried
      e3c2efce: ndt_1c Msg: The OID 0xfd010101 was skippen
      e3c2efce: ndt_1c Msg: Checking if an OID 0xff000000 should be queried
      e3c2efce: ndt_1c Msg: The OID 0xff000000 isn't required, and hence not checked
      e3c2efce: ndt_1c Msg: Checking if an OID 0xff000001 should be queried
      e3c2efce: ndt_1c Msg: The OID 0xff000001 isn't required, and hence not checked
      e3c2efce: ndt_1c Msg: Close adapter
   END TEST: "1c_OIDs", PASSED, Time=1.152
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_OIDs
*** Test ID:        9
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    773
*** Thread Count:   1
*** Execution Time: 0:00:01.152
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=10>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_64BitOIDs
*** Test ID:        10
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    2562
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_64BitOIDs", Threads=0, Seed=2562
      e3c2efce: ndt_1c Msg: Start 1c_64BitOID test on the adapter AX887721
      e3c2efce: ndt_1c Msg: Open adapter
      e3c2efce: ndt_1c Msg: Bind to adapter
      e3c2efce: ndt_1c Msg: Link speed is lower than 1.0Gbps
      e3c2efce: ndt_1c Msg: 64-bit statistics are optional
      e3c2efce: ndt_1c Msg: Querying 64bit OIDs
      e3c2efce: ndt_1c Msg: Query with a null buffer
      e3c2efce: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      e3c2efce: ndt_1c Msg: Query with a four byte buffer
      e3c2efce: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      e3c2efce: ndt_1c Msg: Query with an eight byte buffer
      e3c2efce: ndt_1c Wrn: The miniport should have set BytesWritten to 8 not to 4
      e3c2efce: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      e3c2efce: ndt_1c Msg: Query with a null buffer
      e3c2efce: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      e3c2efce: ndt_1c Msg: Query with a four byte buffer
      e3c2efce: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      e3c2efce: ndt_1c Msg: Query with an eight byte buffer
      e3c2efce: ndt_1c Wrn: The miniport should have set BytesWritten to 8 not to 4
      e3c2efce: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      e3c2efce: ndt_1c Msg: Unbind adapter
      e3c2efce: ndt_1c Msg: Close adapter
   END TEST: "1c_64BitOIDs", PASSED, Time=0.382
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_64BitOIDs
*** Test ID:        10
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    2562
*** Thread Count:   1
*** Execution Time: 0:00:00.382
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=11>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_SuspendResume
*** Test ID:        11
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    8405
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_SuspendResume", Threads=0, Seed=8405
      e3c2efce: ndt_1c Msg: Start 1c_SusRes (Suspend/Resume) test on the adapter AX887721
      e3c2efce: ndt_1c Msg: Enabling the Wake up source : SYSINTR_RTC_ALARM
      e3c2efce: ndt_1c Msg: Suspending the system 1 time
      e3c2efce: ndt_1c Msg: Resumed .....
      e3c2efce: ndt_1c Msg: Sleeping 5 sec .....
      e3c2efce: ndt_1c Msg: Suspending the system 2 time
      e3c2efce: ndt_1c Msg: Resumed .....
      e3c2efce: ndt_1c Msg: Sleeping 10 sec .....
      e3c2efce: ndt_1c Msg: Suspending the system 3 time
      e3c2efce: ndt_1c Msg: Resumed .....
      e3c2efce: ndt_1c Msg: Sleeping 15 sec .....
      e3c2efce: ndt_1c Msg: Suspending the system 4 time
      e3c2efce: ndt_1c Msg: Resumed .....
      e3c2efce: ndt_1c Msg: Sleeping 20 sec .....
      e3c2efce: ndt_1c Msg: Suspending the system 5 time
      e3c2efce: ndt_1c Msg: Resumed .....
      e3c2efce: ndt_1c Msg: Sleeping 25 sec .....
      e3c2efce: ndt_1c Msg: Testing if the adapter AX887721 is fine after suspend/resume
      e3c2efce: ndt_1c Msg: Getting basic info about the adapter
      e3c2efce: ndt_1c Msg: Get OID_GEN_MAXIMUM_TOTAL_SIZE = 1514
      e3c2efce: ndt_1c Msg: Get OID_GEN_MAXIMUM_FRAME_SIZE = 1500
      e3c2efce: ndt_1c Msg: Testing sending to a (random) directed address
      e3c2efce: ndt_1c Msg: Sending 100 packets each of 64 size to a random address
      e3c2efce: ndt_1c Msg: 100 packets were SendCompleted
      e3c2efce: ndt_1c Msg: Sending 100 packets each of 783 size to a random address
      e3c2efce: ndt_1c Msg: 100 packets were SendCompleted
      e3c2efce: ndt_1c Msg: Sending 100 packets each of 1500 size to a random address
      e3c2efce: ndt_1c Msg: 100 packets were SendCompleted
      e3c2efce: ndt_1c Msg: Disabling the Wake up source
   END TEST: "1c_SuspendResume", PASSED, Time=96.143
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_SuspendResume
*** Test ID:        11
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    8405
*** Thread Count:   1
*** Execution Time: 0:01:36.143
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=12>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_StressSusRes
*** Test ID:        12
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    27485
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_StressSusRes", Threads=0, Seed=27485
      e3c2efce: ndt_1c Msg: Start 1c_StressSusRes (Stress in Suspend/Resume) test on the adapter AX887721
      e3c2efce: ndt_1c Msg: Opening adapter
      e3c2efce: ndt_1c Msg: Binding to it
      e3c2efce: ndt_1c Msg: Checking if miniport is PM aware.
      e3c2efce: ndt_1c Msg: AX887721 supports only Power Management, but does not have wake-up capabilities
      43c2ef3e: ndt_1c Msg: StressOIDs: AX887721 supports ** 42 ** OIDs
      43be80c2: ndt_1c Msg: StressSendRecv: stress started
      43c2ef3e: ndt_1c Msg: StressOIDs: stress started
      43be80c2: ndt_1c Msg: StressSendRecv: Sending 1000 packets each of 64 size to a random address
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 1 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 1 time
      e3c2efce: ndt_1c Msg: Waiting 1000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 2 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 2 time
      e3c2efce: ndt_1c Msg: Waiting 1000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 3 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 3 time
      e3c2efce: ndt_1c Msg: Waiting 1000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 4 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 4 time
      e3c2efce: ndt_1c Msg: Waiting 1000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 5 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 5 time
      e3c2efce: ndt_1c Msg: Waiting 1000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 6 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 6 time
      e3c2efce: ndt_1c Msg: Waiting 2000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 7 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 7 time
      e3c2efce: ndt_1c Msg: Waiting 2000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 8 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 8 time
      e3c2efce: ndt_1c Msg: Waiting 2000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 9 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 9 time
      e3c2efce: ndt_1c Msg: Waiting 2000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 10 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 10 time
      e3c2efce: ndt_1c Msg: Waiting 2000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 11 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 11 time
      e3c2efce: ndt_1c Msg: Waiting 4000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 12 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 12 time
      e3c2efce: ndt_1c Msg: Waiting 4000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 13 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 13 time
      e3c2efce: ndt_1c Msg: Waiting 4000 mili sec
      43be80c2: ndt_1c Msg: StressSendRecv: 0 packets each of 64 size were SendCompleted
      43be80c2: ndt_1c Msg: StressSendRecv: Sending 1000 packets each of 127 size to a random address
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 14 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 14 time
      e3c2efce: ndt_1c Msg: Waiting 4000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 15 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 15 time
      e3c2efce: ndt_1c Msg: Waiting 4000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 16 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 16 time
      e3c2efce: ndt_1c Msg: Waiting 5000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 17 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 17 time
      e3c2efce: ndt_1c Msg: Waiting 5000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 18 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 18 time
      e3c2efce: ndt_1c Msg: Waiting 5000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 19 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 19 time
      e3c2efce: ndt_1c Msg: Waiting 5000 mili sec
      e3c2efce: ndt_1c Msg: Transitioning the adapter to D4 state 20 time
      e3c2efce: ndt_1c Msg: Transitioning back to D0 state 20 time
      e3c2efce: ndt_1c Msg: Waiting 5000 mili sec
      e3c2efce: ndt_1c Msg: Waiting for Stress OIDs thread to terminate
      43c2ef3e: ndt_1c Msg: StressOIDs: signaled to stop
      43c2ef3e: ndt_1c Msg: StressOIDs: Cleaned up & exiting.
      e3c2efce: ndt_1c Msg: Stress OIDs thread exited with exit value : PASS
      e3c2efce: ndt_1c Msg: Waiting for StressSendRecv thread to terminate
      43be80c2: ndt_1c Msg: StressSendRecv: 80 packets each of 127 size were SendCompleted
      43be80c2: ndt_1c Msg: StressSendRecv: signaled to stop
      43be80c2: ndt_1c Msg: StressSendRecv: Cleaned up & exiting.
      e3c2efce: ndt_1c Msg: Stress SendRecv thread exited with exit value : PASS
      e3c2efce: ndt_1c Msg: Unbinding to it
      e3c2efce: ndt_1c Msg: Closing adapter
   END TEST: "1c_StressSusRes", PASSED, Time=110.541
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_StressSusRes
*** Test ID:        12
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    27485
*** Thread Count:   1
*** Execution Time: 0:01:50.541
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=13>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_ResetOnResume
*** Test ID:        13
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Random Seed:    24257
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_ResetOnResume", Threads=0, Seed=24257
      e3c2efce: ndt_1c Msg: Start 1c_ResetOnResume (Reset on Resume) test on the adapter AX887721
      e3c2efce: ndt_1c Msg: This test will test if AX887721 restores its settings after Reset
      e3c2efce: ndt_1c Msg: AX887721 supports only Power Management, but does not have wake-up capabilities
      e3c2efce: ndt_1c Msg: Set CURRENT_PACKET_FILTER = NDIS_PACKET_TYPE_MULTICAST|NDIS_PACKET_TYPE_DIRECTED for adapter AX887721
      e3c2efce: ndt_1c Msg: AX887721 supports max 64 Multicast addresses
      e3c2efce: ndt_1c Msg: Got the current complete list of multicast addresses for AX887721
      e3c2efce: ndt_1c Msg: It has 0 multicast addresses set
      e3c2efce: ndt_1c Msg: Set 62 multicast addresses for AX887721
      e3c2efce: ndt_1c Msg: We'll RESET the device & at the end of every RESET we'll verify if AX887721 restores its settings or not
      e3c2efce: ndt_1c Msg: Reseting the network adapter AX887721 1 time
      e3c2efce: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX887721
      e3c2efce: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX887721
      e3c2efce: ndt_1c Msg: AX887721 has restored/retained its Packet Filter settings.
      e3c2efce: ndt_1c Msg: AX887721 has restored/retained its multicast addresses list.
      e3c2efce: ndt_1c Msg: AX887721 has passed ResetOnResume test
      e3c2efce: ndt_1c Msg: Reseting the network adapter AX887721 2 time
      e3c2efce: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX887721
      e3c2efce: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX887721
      e3c2efce: ndt_1c Msg: AX887721 has restored/retained its Packet Filter settings.
      e3c2efce: ndt_1c Msg: AX887721 has restored/retained its multicast addresses list.
      e3c2efce: ndt_1c Msg: AX887721 has passed ResetOnResume test
      e3c2efce: ndt_1c Msg: Reseting the network adapter AX887721 3 time
      e3c2efce: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX887721
      e3c2efce: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX887721
      e3c2efce: ndt_1c Msg: AX887721 has restored/retained its Packet Filter settings.
      e3c2efce: ndt_1c Msg: AX887721 has restored/retained its multicast addresses list.
      e3c2efce: ndt_1c Msg: AX887721 has passed ResetOnResume test
      e3c2efce: ndt_1c Msg: Reseting the network adapter AX887721 4 time
      e3c2efce: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX887721
      e3c2efce: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX887721
      e3c2efce: ndt_1c Msg: AX887721 has restored/retained its Packet Filter settings.
      e3c2efce: ndt_1c Msg: AX887721 has restored/retained its multicast addresses list.
      e3c2efce: ndt_1c Msg: AX887721 has passed ResetOnResume test
      e3c2efce: ndt_1c Msg: Reseting the network adapter AX887721 5 time
      e3c2efce: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX887721
      e3c2efce: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX887721
      e3c2efce: ndt_1c Msg: AX887721 has restored/retained its Packet Filter settings.
      e3c2efce: ndt_1c Msg: AX887721 has restored/retained its multicast addresses list.
      e3c2efce: ndt_1c Msg: AX887721 has passed ResetOnResume test
   END TEST: "1c_ResetOnResume", PASSED, Time=11.061
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_ResetOnResume
*** Test ID:        13
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX887721
*** Result:         Passed
*** Random Seed:    24257
*** Thread Count:   1
*** Execution Time: 0:00:11.061
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
END GROUP: ndt_1c.dll
*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:    24,092,672 bytes
*** Memory Used:      8,478,720 bytes
*** Memory Free:     15,613,952 bytes
***
*** Kernel Used:        708,608 bytes
*** Water Mark:           3,757 pages
***
*** Store Total:     24,027,136 bytes
*** Store Used:         595,088 bytes
*** Store Free:      23,432,048 bytes
*** ==================================================================

*** ==================================================================
*** SUITE SUMMARY
***
*** Passed:         12
*** Failed:          0
*** Skipped:         1
*** Aborted:         0
*** -------- ---------
*** Total:          13
***
*** Cumulative Test Execution Time: 0:14:44.783
*** Total Tux Suite Execution Time: 0:14:47.962
*** CPU Idle Time:                  0:12:50.933
*** ==================================================================
</TESTGROUP>
@@@@@@0

