## Izvēlņu pārskats

Vadības panelis sniedz piekļuvi vairākām izvēlnēm, lai iestatītu ierīci vai izmantotu ierīces funkcijas.

- Šī funkcija netiek atbalstīta modelim SCX-340x/SCX-340xW Series (sk. Vadības paneļa pārskats).

- Atkarībā no opcijām vai modeļiem dažas izvēlnes, iespējams, displejā netiks parādītas. Ja tā ir, tās neattiecas uz jūsu ierīci.

- Dažu izvēlņu nosaukumi var atšķirties no jūsu ierīces nosaukumiem atkarībā no tās opcijām vai modeļa.

- Informācija par izvēlnēm ir papildu rokasgrāmatā (sk. Noderīgu iestatījumu izvēlnes).

### Piekļūšana izvēlnei

1. Atkarībā no izmantojamās funkcijas atlasiet vadības paneļa pogu Fax, Copy vai Scan.

2. Atlasiet (Menu), līdz displeja apakšējā rindā tiek parādīta vajadzīgā izvēlne, un nospiedietOK.

3. Spiediet bultiņas, līdz tiek parādīts vajadzīgais izvēlnes vienums, un nospiediet OK.

4. Ja iestatījuma vienumam ir apakšizvēlnes, atkārtojiet 3. darbību.

5. Nospiediet pogu OK, lai saglabātu atlasi.

6. Nospiediet (Stop/Clear), lai atgrieztos gatavības režīmā.

Vienumi | Opcijas
--- | ---
Fax Feature | Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Resolution | Standard Fine Super Fine Photo Fax Color Fax
Scan Size
Multi Send
Delay Send
Fax Feature (turpinājums) | Priority Send
Forward | Fax PC
Secure Receive | Off On Print
Add Page
Cancel Job

Fax Setup

Sending

Redial Times

Redial Term

Prefix Dial

ECM Mode

Send Report

Image TCR

Dial Mode [a]

Fax Setup (turpinājums)

Receiving

Receive Mode

Ring To Answer

Stamp RCV Name

RCV Start Code

Auto Reduction

Discard Size

Junk Fax Setup

DRPD Mode [a]

Change Default | Resolution Darkness Contrast Scan Size
Auto Report | On Off
Copy Feature | Scan Size
Reduce/Enlarge
Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Copy Feature (turpinājums) | Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Original Type | Text Text/Photo Photo

Layout

Normal

2-Up

4-Up

ID Copy

Poster Copy

Clone Copy

Adjust Bkgd. | Off Auto Enhance Lev.1 Enhance Lev.2 Erase Lev.1- Erase Lev.4

Copy Setup

Change Default

Scan Size

Copies

Copy Collation

Reduce/Enlarge

Darkness

Contrast

Original Type

Adjust Bkgd.

System Setup

Machine Setup

Machine ID

Fax Number

Date & Time

Clock Mode

Language

Power Save

Wakeup Event

System Timeout

Altitude Adj.

Auto Continue [b]

Paper Mismatch

Paper Substit. [b]

Toner Save

Eco Settings

Paper Setup | Paper Size Paper Type Margin
System Setup (turpinājums) | Sound/Volume | Key Sound Alarm Sound Speaker Ringer

Report

All Report

Configuration

Supplies Info.

Address Book

Fax Send

Fax Sent

Fax Received

Schedule Jobs

Junk Fax

Network Conf. [c]

Usage Counter

Fax Options

Maintenance | CLR Empty Msg. [d] Supplies Life Serial No. TonerLow Alert

System Setup (turpinājums)

Clear Setting

All Settings

Fax Setup

Copy Setup

System Setup

Network Setup [c]

Address Book

Fax Sent

Fax Received

Network [c] | TCP/IP (IPv4) | DHCP BOOTP Static
TCP/IP (IPv6) | IPv6 Activate DHCPv6 Config
Ethernet Speed | Automatic 10Mbps Half 10Mbps Full 100Mbps Half 100Mbps Full

Network [c] (turpinājums)

Wireless

Wi-Fi ON/OFF

Wi-Fi Direct

WPS Setting

WLAN Setting

WLAN Default

WLAN Signal

Clear Setting
Network Conf.
[a] Atkarībā no valsts šī opcija, iespējams, nebūs pieejama. [b] Šī opcija parādās tikai tad, kad ir iespējota funkcija Paper Mismatch. [c] Tikai SCX-340xFW/SCX-340xHW Series. [d] Šī opcija parādās tikai tad, ja kasetnē ir palicis maz tonera.