## Meniu apžvalga

Valdymo skydelis užtikrina prieigą prie įvairių meniu, skirtų aparatui parengti, arba aparato funkcijoms naudoti.

- Ši funkcija nepalaikoma SCX-340x/SCX-340xW Series (žr. Valdymo skydelio apžvalga).

- Atsižvelgiant į parinktis ar modelius kai kurių meniu ekrane gali ir nebūti. Tokiu atveju tai reiškia, kad jie netaikomi jūsų aparatui.

- Kai kurie meniu pavadinimai gali skirtis nuo jūsų įrenginio meniu pavadinimų, priklausomai nuo įrenginio funkcijų ar modelio.

- Meniu aprašyti Papildomos informacijos vadove (žr. Naudingi nustatymų meniu).

### Meniu įjungimas

1. Paspauskite valdymo skydelyje esantį norimos naudoti funkcijos mygtuką „Fax“, „Copy“ arba „Scan“.

2. Spaudykite (Menu) kol apatinėje ekrano eilutėje pasirodys norimas meniu ir spauskite OK.

3. Spauskite rodykles tol, kol bus parodytas reikiamas meniu punktas, tuomet paspauskite OK.

4. Jei nustatymas turi submeniu, kartokite 3 žingsnį.

5. Paspauskite OK, kad išsaugotumėte pasirinkimą.

6. Paspauskite (Stop/Clear), kad grįžtumėte į parengties režimą.

Elementai | Parinktys
--- | ---
Fax Feature | Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Resolution | Standard Fine Super Fine Photo Fax Color Fax
Scan Size
Multi Send
Delay Send
Fax Feature (tęsinys) | Priority Send
Forward | Fax PC
Secure Receive | Off On Print
Add Page
Cancel Job

Fax Setup

Sending

Redial Times

Redial Term

Prefix Dial

ECM Mode

Send Report

Image TCR

Dial Mode [a]

Fax Setup (tęsinys)

Receiving

Receive Mode

Ring To Answer

Stamp RCV Name

RCV Start Code

Auto Reduction

Discard Size

Junk Fax Setup

DRPD Mode [a]

Change Default | Resolution Darkness Contrast Scan Size
Auto Report | On Off
Copy Feature | Scan Size
Reduce/Enlarge
Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Copy Feature (Tęsti) | Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Original Type | Text Text/Photo Photo

Layout

Normal

2-Up

4-Up

ID Copy

Poster Copy

Clone Copy

Adjust Bkgd. | Off Auto Enhance Lev.1 Enhance Lev.2 Erase Lev.1- Erase Lev.4

Copy Setup

Change Default

Scan Size

Copies

Copy Collation

Reduce/Enlarge

Darkness

Contrast

Original Type

Adjust Bkgd.

System Setup

Machine Setup

Machine ID

Fax Number

Date & Time

Clock Mode

Language

Power Save

Wakeup Event

System Timeout

Altitude Adj.

Auto Continue [b]

Paper Mismatch

Paper Substit. [b]

Toner Save

Eco Settings

Paper Setup | Paper Size Paper Type Margin
System Setup (tęsinys) | Sound/Volume | Key Sound Alarm Sound Speaker Ringer

Report

All Report

Configuration

Supplies Info.

Address Book

Fax Send

Fax Sent

Fax Received

Schedule Jobs

Junk Fax

Network Conf. [c]

Usage Counter

Fax Options

Maintenance | CLR Empty Msg. [d] Supplies Life Serial No. TonerLow Alert

System Setup (tęsinys)

Clear Setting

All Settings

Fax Setup

Copy Setup

System Setup

Network Setup [c]

Address Book

Fax Sent

Fax Received

Network [c] | TCP/IP (IPv4) | DHCP BOOTP Static
TCP/IP (IPv6) | IPv6 Activate DHCPv6 Config
Ethernet Speed | Automatic 10Mbps Half 10Mbps Full 100Mbps Half 100Mbps Full

Network [c] (Tęsti)

Wireless

Wi-Fi ON/OFF

Wi-Fi Direct

WPS Setting

WLAN Setting

WLAN Default

WLAN Signal

Clear Setting
Network Conf.
[a] Atsižvelgiant į šalį šios parinkties gali nebūti. [b] Ši parinktis rodoma tik tada, kai įjungta parinktis Paper Mismatch. [c] tik SCX-340xFW/SCX-340xHW Series. [d] Ši parinktis rodoma tik tuomet, kai kasetėje lieka nedaug dažų.