## مروری بر منو

پانل کنترل دسترسی به منوهای مختلف جهت تنظیم دستگاه یا استفاده از عملکردهای دستگاه را در اختیار شما قرار می دهد.

- این قابلیت برای مدل های SCX-340x/SCX-340xW Series وجود ندارد (به نمای کلی پانل کنترل رجوع کنید).

- بسته به گزینه ها یا مدل ها ممکن است بعضی از منوها بدرستی بر روی صفحه نشان داده نشود. در اینصورت، آن مورد در دستگاه شما قابل استفاده نیست.

- نام بعضی از منوها بسته به امکانات اختیار یا مدل دستگاه، ممکن است متفاوت با نام آنها در ماشین شما باشد.

- منوها در قسمت راهنمای پیشرفته توضیح داده شده اند (رجوع کنید به منوهای تنظيمات مفيد).

### دسترسی به منو

1. دکمه Fax، Copy، يا Scan را بسته به قابليتی که قرار است استفاده شود از روی صفحه کنترل انتخاب کنيد.

2. (Menu) را فشار دهيد تا فهرست مورد نظر شما در سطر پايين صفحه نمايش ظاهر شود و OK را فشار دهيد.

3. برای ظاهر شدن آيتم منوی مورد نظر، فلش ها را فشار داده و سپس OK کلیک کنید.

4. در صورتی که اين آيتم تنظيم دارای زير فهرست است، مرحله 3 را تکرار کنيد.

5. OK را برای ذخیره انتخاب خود فشار دهید.

6. برای بازگشت به حالت آماده، دکمه (Stop/Clear) را فشار دهید.

موارد | گزینه ها
--- | ---
Fax Feature | Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Resolution | Standard Fine Super Fine Photo Fax Color Fax
Scan Size
Multi Send
Delay Send
Fax Feature (ادامه) | Priority Send
Forward | Fax PC
Secure Receive | Off On Print
Add Page
Cancel Job

Fax Setup

Sending

Redial Times

Redial Term

Prefix Dial

ECM Mode

Send Report

Image TCR

Dial Mode [a]

Fax Setup (ادامه)

Receiving

Receive Mode

Ring to Answer

Stamp RCV Name

RCV Start Code

Auto Reduction

Discard Size

Junk Fax Setup

DRPD Mode [a]

Change Default | Resolution Darkness Contrast Scan Size
Auto Report | On Off
Copy Feature | Scan Size
Reduce/Enlarge
Darkness | Normal Dark+1- Dark+5 Contrast
Copy Feature (ادامه) | کنتراست | Normal Dark+1- Dark+5 Light+5- Light+1
Original Type | Text Text/Photo Photo

Layout

Normal

2-Up

4-Up

ID Copy

Poster Copy

Clone Copy

Adjust Bkgd.‎ | Off Auto Enhance Lev.1 Enhance Lev.2 Erase Lev.1- Erase Lev.4

Copy Setup

Change Default

Scan Size

Copies

Copy Collation

Reduce/Enlarge

Darkness

Contrast

Original Type

Adjust Bkgd.‎

System Setup

Machine Setup

Machine ID

Fax Number

Date & Time

Clock Mode

Language

Power Save

Wakeup Event

System Timeout

‎Altitude Adj.‎

‏‏Auto Continue [b]

Paper Mismatch

Paper Substit.‎ [b]

Toner Save

Eco Settings

Paper Setup | Paper Size Paper Type Margin
System Setup (ادامه) | Sound/Volume | Key Sound Alarm Sound Speaker Ringer

Report

All Report

Configuration

‎Supplies Info.‎

Address Book

Fax Send

Fax Sent

Fax Received

Schedule Jobs

Junk Fax

‏‏‏Network Conf.‎ [c]

Usage Counter

Fax Options

Maintenance | ‏‏‏CLR Empty Msg.‎ [d] Supplies Life Serial No. TonerLow Alert

System Setup (ادامه)

Clear Setting

All Settings

Fax Setup

Copy Setup

System Setup

‏Network Setup [c]

Address Book

Fax Sent

Fax Received

Network [c] | TCP/IP (IPv4)‎ | DHCP BOOTP Static
TCP/IP (IPv6)‎ | IPv6 Activate DHCPv6 Config
Ethernet Speed | Automatic 10Mbps Half 10Mbps Full 100Mbps Half 100Mbps Full

Network [c] (ادامه)

Wireless

Wi-Fi ON/OFF

Wi-Fi Direct

WPS Setting

WLAN Setting

WLAN Default

WLAN Signal

Clear Setting
‏‏‏Network Conf.‎
[a] این گزینه ممکن است بسته به کشور شما موجود نباشد. [b] ‏این گزینه تنها وقتی Paper Mismatch فعال باشد، ظاهر می شود. [c] فقط SCX-340xFW/SCX-340xHW Series. [d] ‏این گزینه تنها وقتی ظاهر می شود که مقدار کمی تونر در کارتریج باقی مانده باشد.