## Tinjauan menu

Panel kontrol menyediakan akses ke berbagai menu untuk menyetel mesin atau menggunakan berbagai fungsi mesin.

- Fungsi ini tidak tersedia untuk SCX-340x/SCX-340xW Series (lihat Tinjauan panel kontrol).

- Beberapa menu mungkin tidak akan muncul pada layar tergantung pada opsi atau modelnya. Jika demikian, menu itu tidak berlaku pada printer Anda.

- Beberapa nama menu mungkin berbeda dengan printer Anda tergantung pada opsi atau modelnya.

- Menu tersebut diterangkan dalam Panduan Tingkat Lanjut (lihat Menu Pengaturan Yang Berguna).

### Mengakses menu

1. Pilih tombol Faks, Fotokopi, atau Pemindaian pada panel kontrol tergantung pada fitur yang digunakan.

2. Pilih (Menu) hingga menu yang dikehendaki muncul di baris terbawah pada tampilan, kemudian tekan OK.

3. Tekan panah sampai item menu yang Anda butuhkan ditampilkan, kemudian tekan OK.

4. Jika item penyetelan memiliki sub menu, ulangi langkah 3.

5. Tekan OK untuk menyimpan pilihan Anda.

6. Tekan (Stop/Clear) untuk kembali ke mode siap.

Item | Opsi
--- | ---
Fax Feature | Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Resolution | Standard Fine Super Fine Photo Fax Color Fax
Scan Size
Multi Send
Delay Send
Fax Feature (Lanjutan) | Priority Send
Forward | Fax PC
Secure Receive | Off On Print
Add Page
Cancel Job

Fax Setup

Sending

Redial Times

Redial Term

Prefix Dial

ECM Mode

Send Report

Image TCR

Dial Mode [a]

Fax Setup (Lanjutan)

Receiving

Receive Mode

Ring To Answer

Stamp RCV Name

RCV Start Code

Auto Reduction

Discard Size

Junk Fax Setup

DRPD Mode [a]

Change Default | Resolution Darkness Contrast Scan Size
Auto Report | On Off
Copy Feature | Scan Size
Reduce/Enlarge
Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Copy Feature (Bersambung) | Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Original Type | Text Text/Photo Photo

Layout

Normal

2-Up

4-Up

ID Copy

Poster Copy

Clone Copy

Adjust Bkgd. | Off Auto Enhance Lev.1 Enhance Lev.2 Erase Lev.1- Erase Lev.4

Copy Setup

Change Default

Scan Size

Copies

Copy Collation

Reduce/Enlarge

Darkness

Contrast

Original Type

Adjust Bkgd.

System Setup

Machine Setup

Machine ID

Fax Number

Date & Time

Clock Mode

Language

Power Save

Wakeup Event

System Timeout

Altitude Adj.

Auto Continue [b]

Paper Mismatch

Paper Substit. [b]

Toner Save

Eco Settings

Paper Setup | Paper Size Paper Type Margin
System Setup (Lanjutan) | Sound/Volume | Key Sound Alarm Sound Speaker Ringer

Report

All Report

Configuration

Supplies Info.

Address Book

Fax Send

Fax Sent

Fax Received

Schedule Jobs

Junk Fax

Network Conf. [c]

Usage Counter

Fax Options

Maintenance | CLR Empty Msg. [d] Supplies Life Serial No. TonerLow Alert

System Setup (Lanjutan)

Clear Setting

All Settings

Fax Setup

Copy Setup

System Setup

Network Setup [c]

Address Book

Fax Sent

Fax Received

Network [c] | TCP/IP (IPv4) | DHCP BOOTP Static
TCP/IP (IPv6) | IPv6 Activate DHCPv6 Config
Ethernet Speed | Automatic 10Mbps Half 10Mbps Full 100Mbps Half 100Mbps Full

Network [c] (Bersambung)

Wireless

Wi-Fi ON/OFF

Wi-Fi Direct

WPS Setting

WLAN Setting

WLAN Default

WLAN Signal

Clear Setting
Network Conf.
[a] Opsi ini mungkin tidak tersedia, tergantung negara. [b] Opsi ini hanya muncul jika Paper Mismatch diaktifkan. [c] SCX-340xFW/SCX-340xHW Series saja. [d] Opsi ini hanya muncul bila toner masih tersisa sedikit di dalam kartrid.