## Prehľad ponúk

Ovládací panel zabezpečuje prístup do rôznych ponúk na nastavenie zariadenia alebo na použitie jeho funkcií.

- Zariadenia SCX-340x/SCX-340xW Series nepodporujú túto funkciu (pozri Ovládací panel – prehľad).

- V závislosti od možností a modelov sa niektoré ponuky nemusia na displeji zobrazovať. V takom prípade sa nevzťahujú na vaše zariadenie.

- Niektoré názvy v ponukách sa môžu od vášho zariadenia líšiť v závislosti od doplnkov a modelu.

- Ponuky sú opísané v Pokročilej príručke (pozri Užitočné ponuky na nastavenie).

### Prístup do menu

1. V závislosti od funkcie, ktorú chcete použiť zvoľte na ovládacom paneli tlačidlo faxovania, kopírovania alebo skenovania.

2. Stláčajte (Menu), kým sa v spodnom riadku displeja neobjaví požadovaná ponuka a potom stlačte OK.

3. Stláčajte tlačidlá šípiek, až kým sa nezobrazí požadovaná položka ponuky a stlačte tlačidlo OK.

4. Ak položka ponuky obsahuje ďalšie podponuky, opakujte krok 3.

5. Stlačením OK uložte výber.

6. Stlačením tlačidla (Stop/Clear) sa vráťte do pohotovostného režimu.

Položky | Voľby
--- | ---
Fax Feature | Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Resolution | Standard Fine Super Fine Photo Fax Color Fax
Scan Size
Multi Send
Delay Send
Fax Feature (pokračovanie) | Priority Send
Forward | Fax PC
Secure Receive | Off On Print
Add Page
Cancel Job

Fax Setup

Sending

Redial Times

Redial Term

Prefix Dial

ECM Mode

Send Report

Image TCR

Dial Mode [a]

Fax Setup (pokračovanie)

Receiving

Receive Mode

Ring To Answer

Stamp RCV Name

RCV Start Code

Auto Reduction

Discard Size

Junk Fax Setup

DRPD Mode [a]

Change Default | Resolution Darkness Contrast Scan Size
Auto Report | On Off
Copy Feature | Scan Size
Reduce/Enlarge
Darkness | Normal Dark+1- Dark+5 Light+5- Light+1
Copy Feature (Pokračovanie) | Contrast | Normal Dark+1- Dark+5 Light+5- Light+1
Original Type | Text Text/Photo Photo

Layout

Normal

2-Up

4-Up

ID Copy

Poster Copy

Clone Copy

Adjust Bkgd. | Off Auto Enhance Lev.1 Enhance Lev.2 Erase Lev.1- Erase Lev.4

Copy Setup

Change Default

Scan Size

Copies

Copy Collation

Reduce/Enlarge

Darkness

Contrast

Original Type

Adjust Bkgd.

System Setup

Machine Setup

Machine ID

Fax Number

Date & Time

Clock Mode

Language

Power Save

Wakeup Event

System Timeout

Altitude Adj.

Auto Continue [b]

Paper Mismatch

Paper Substit. [b]

Toner Save

Eco Settings

Paper Setup | Paper Size Paper Type Margin
System Setup (pokračovanie) | Sound/Volume | Key Sound Alarm Sound Speaker Ringer

Report

All Report

Configuration

Supplies Info.

Address Book

Fax Send

Fax Sent

Fax Received

Schedule Jobs

Junk Fax

Network Conf. [c]

Usage Counter

Fax Options

Maintenance | CLR Empty Msg. [d] Supplies Life Serial No. TonerLow Alert

System Setup (pokračovanie)

Clear Setting

All Settings

Fax Setup

Copy Setup

System Setup

Network Setup [c]

Address Book

Fax Sent

Fax Received

Network [c] | TCP/IP (IPv4) | DHCP BOOTP Static
TCP/IP (IPv6) | IPv6 Activate DHCPv6 Config
Ethernet Speed | Automatic 10Mbps Half 10Mbps Full 100Mbps Half 100Mbps Full

Network [c] (Pokračovanie)

Wireless

Wi-Fi ON/OFF

Wi-Fi Direct

WPS Setting

WLAN Setting

WLAN Default

WLAN Signal

Clear Setting
Network Conf.
[a] V niektorých krajinách nemusí byť táto voľba k dispozícii. [b] Táto možnosť sa zobrazí len v prípade, ak ste zapli funkciu Paper Mismatch. [c] Len SCX-340xFW/SCX-340xHW Series. [d] Táto možnosť sa zobrazí len v prípade, ak v kazete zostalo malé množstvo tonera.